# --- Session Options
#
# Note:                    X is a number equal to or greater than 0
#
# SESSION_TITLE            Title description for SESSION
# SESSION_TYPE             Package type, choose beetwen:
#                          - vncviewer        Start vncviewer in X
#                          - rdesktop         Start rdesktop in X
#                          - x                Start x-terminal session (xdm)
#                          - ssh              Start ssh client in linux console
#                          - telnet           Start telnet client in linux console
#                          - ica              Start Citrix ICA client in X
#                          - tn5250           Start AS400 client in linux console
# SESSION_[PACKAGE]_SERVER   IP address/hostname of the server
# SESSION_[PACKAGE]_OPTIONS  Command line options for the session type




# Imporatant: You can have multiple sessions, but make sure you start at SESSION 0.
# Otherwise you will get an error on boot.

# If you only have one session, it is a good idea to uncomment this line:

AUTOSTART=On

#SESSION_0_TITLE="TESTE MASCARA"
SESSION_0_TYPE=rdesktop
SESSION_0_RDESKTOP_SERVER=192.168.0.200
SESSION_0_RDESKTOP_OPTIONS="-a 16"


# Note: use '-a 16' and '-a 24' to get true-color with Windows 2003+
# Older servers don't support these color depths, wrong settings may cause connection to fail.
#SESSION_1_TITLE="Windows 2003 terminal server (16 bit color depth)"
#SESSION_1_TYPE=rdesktop
#SESSION_1_RDESKTOP_SERVER=192.168.0.200
#SESSION_1_RDESKTOP_OPTIONS="-u user -p password -a 16"



# --- General Options
#
# KEYBOARD_MAP       Keyboard layout
# TIME_ZONE          Used to set time zone on TS client
# AUTOPLAYCD         If enabled this will autoplay music cds when inserted.
# RECONNECT_PROMPT   Will prompt for reconnection to server, otherwise Autoconnects, On/Off

KEYBOARD_MAP=pt_br
#TIME_ZONE=US
#AUTOPLAYCD=On
RECONNECT_PROMPT=Off


# --- XServer Options
#
# SCREEN_RESOLUTION       Screen resolutions available in the workstations
# SCREEN_COLOR_DEPTH      Number of bits per pixel (8,16,24)
# SCREEN_HORIZSYNC        Monitor horizontal sync frequency in Khz.
# SCREEN_VERTREFRESH      Monitor vertical refresh frecuency in Hz.
# SCREEN_X_FONT_SERVER    IP address or hostname of the font server for X
# MOUSE_PROTOCOL          Mouse protocol type (Microsoft, PS/2, etc.)
#                         (mouse is autodetected, use this only if it fails)
# MOUSE_DEVICE            Mouse device:  /dev/ttyS0 -> COM1
#                                   /dev/ttyS1 -> COM2
#                                   /dev/ttyS2 -> COM3
#                                   /dev/ttyS3 -> COM4
#                                   /dev/psaux -> PS/2 mouse port
#                                   /dev/input/mice -> USB mouse (needs USB package)
# MOUSE_RESOLUTION        Mouse resolution

#SCREEN_RESOLUTION="800x600"
SCREEN_RESOLUTION="1024x768"

SCREEN_COLOR_DEPTH="16"
#SCREEN_HORIZSYNC="30-64"

SCREEN_HORIZSYNC="31.47, 35.16, 35.52, 37.5, 46.9, 60"
SCREEN_VERTREFRESH="56-87"



#SCREEN_X_FONT_SERVER=192.168.1.2:7100
#MOUSE_PROTOCOL=PS/2
#MOUSE_DEVICE=/dev/psaux
MOUSE_RESOLUTION=100

# --- Printing Options
#
# PRINTER_0_NAME     Workstation Printer Name, Can be Any Valid Name
# PRINTER_0_DEVICE   Workstation printer device (if not specified devices
#                    are not loaded).
#                       /dev/printers/[0-2]   for parallel ports
#                       /dev/ttyS[0-3] for serial ports
#                       /dev/usb/lp[0-2] for USB printers
#
# PRINTER_0_TYPE     N for network, P for parallel, S for serial, U for USB printer
# PRINTER_0_OPTIONS  Serial port options.
# PRINTER_1_*        See PRINTER_0_*
# PRINTER_2_*        See PRINTER_0_*
# PRINTER_3_*        See PRINTER_0_*

#PRINTER_0_NAME=parallel
#PRINTER_0_DEVICE=/dev/printers/0
#PRINTER_0_TYPE=P

#PRINTER_1_NAME=serial
#PRINTER_1_DEVICE=/dev/ttyS1
#PRINTER_1_TYPE=S
#PRINTER_1_OPTIONS="speed 38400 -imaxbel"

#PRINTER_2_NAME=usb
#PRINTER_2_DEVICE=/dev/usb/lp0
#PRINTER_2_TYPE=U


